S.1 Camy Edge Detection

1. Pick a real image or take a photo
   1. Convert to ppm on jupyterhub
   2. Make sure the photo is not square
   3. Input: image.ppm
2. Calculate intensity
   1. (R+G+B)/3
   2. Create imageg.ppm
      1. Grayscale image